{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":9,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","","FCAHG71FVEB (Archived)","FCAHG100FVEB (Archived)","FCAHG125FVEB (Archived)","FCAHG140FVEB (Archived)"]
["Περίβλημα","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","288","288","288","288"]
["","","","Πλάτος","mm","840","840","840","840"]
["","","","Βάθος","mm","840","840","840","840"]
["Βάρος","Μονάδα","","","kg","25.0","26.0","26.0","26.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","21.2","32.3","33.5","33.5"]
["","","","Μέτρια","m³/min","16.7","25.7","26.7","27.3"]
["","","","Χαμηλή","m³/min","12.2","19.0","19.9","21.1"]
["","","Θέρμανση","Υψ.","m³/min","21.2","32.3","33.5","33.5"]
["","","","Μέτρια","m³/min","16.7","25.7","26.7","27.3"]
["","","","Χαμηλή","m³/min","12.2","19.0","19.9","21.1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53","61","61","61"]
["","Θέρμανση","","","dBA","53","61","61","61"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","36","44","45","45"]
["","","","Μέτρια","dBA","33","39","40","41"]
["","","","Χαμηλή","dBA","29","33","35","37"]
["","Θέρμανση","","Υψ.","dBA","36","44","45","45"]
["","","","Μέτρια","dBA","33","39","40","41"]
["","","","Χαμηλή","dBA","29","33","35","37"]
["Ψυκτικό μέσο","GWP","","","","675","675","675","675"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","15.9","15.9","15.9","15.9"]
["","Αποχέτευση","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Διακοσμητική μάσκα","Μοντέλο","","","","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα"]
["","Χρώμα","","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Ύψος","mm","130","130","130","130"]
["","","","Πλάτος","mm","950","950","950","950"]
["","","","Βάθος","mm","950","950","950","950"]
["","Βάρος","","","kg","10","10","10","10"]
["Διακοσμητική μάσκα 2","Μοντέλο","","","","BYCQ140D7GW1 - Μάσκα αυτοκαθαρισμού","BYCQ140D7GW1 - Μάσκα αυτοκαθαρισμού","BYCQ140D7GW1 - Μάσκα αυτοκαθαρισμού","BYCQ140D7GW1 - Μάσκα αυτοκαθαρισμού"]
["","Χρώμα","","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Ύψος","mm","130","130","130","130"]
["","","","Διακοσμητική μάσκα 2-=-Διαστάσεις-=-Πλάτος-=-mm","mm","950","950","950","950"]
["","","","Διακοσμητική μάσκα 2-=-Διαστάσεις-=-Βάθος-=-mm","mm","950","950","950","950"]
["","Βάρος","","","kg","10.3","10.3","10.3","10.3"]
["Διακοσμητική μάσκα 3","Μοντέλο","","","","BYCQ140D7W1W - Εντελώς λευκή, Βλ. σημείωση 1","BYCQ140D7W1W - Εντελώς λευκή, Βλ. σημείωση 1","BYCQ140D7W1W - Εντελώς λευκή, Βλ. σημείωση 1","BYCQ140D7W1W - Εντελώς λευκή, Βλ. σημείωση 1"]
["","Χρώμα","","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Διακοσμητική μάσκα 3-=-Διαστάσεις-=-Ύψος-=-mm","mm","50","50","50","50"]
["","","","Διακοσμητική μάσκα 3-=-Διαστάσεις-=-Πλάτος-=-mm","mm","950","950","950","950"]
["","","","Διακοσμητική μάσκα 3-=-Διαστάσεις-=-Βάθος-=-mm","mm","950","950","950","950"]
["","Βάρος","","","kg","5.4","5.4","5.4","5.4"]
["Διακοσμητική μάσκα 4","Μοντέλο","","","","BYCQ140D7W1 - Λευκή με γκρίζα πτερύγια","BYCQ140D7W1 - Λευκή με γκρίζα πτερύγια","BYCQ140D7W1 - Λευκή με γκρίζα πτερύγια","BYCQ140D7W1 - Λευκή με γκρίζα πτερύγια"]
["","Χρώμα","","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Διακοσμητική μάσκα 4-=-Διαστάσεις-=-Ύψος-=-mm","mm","50","50","50","50"]
["","","","Διακοσμητική μάσκα 4-=-Διαστάσεις-=-Πλάτος-=-mm","mm","950","950","950","950"]
["","","","Διακοσμητική μάσκα 4-=-Διαστάσεις-=-Βάθος-=-mm","mm","950","950","950","950"]
["","Βάρος","","","kg","5.4","5.4","5.4","5.4"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης"]
["","Εγχειρίδιο εγκατάστασης και χειρισμού","","","","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού"]
["Τροφοδοσία ισχύος","Όνομα","","","","VE","VE","VE","VE"]
["","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται."]
["","","","","","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]