{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Απόδοση ψύξης","Ονομ.","","kW","","","","","","","6.80","6.80","13.40"]
["Ψύξη χώρου","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","345","345","1,191"]
["","Απόδοση","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","A++","A++"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","A+","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Ονομαστική απόδοση","EER","","","","","","","","","4.09","4.09","3.18"]
["Σημειώσεις","","","","","","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","","","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","","","","","","","A"]
["","","Θέρμανση","","","","","","","","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","","","","","","","7.50","15.50"]
["Σημειώσεις","","","","","","","","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","","","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Ψύξη χώρου","ηs, c","","%","","","","","","","","","266.88"]
["Θέρμανση χώρου (Μέσο κλίμα)","ηs,h","","%","","","","","","","","","172.10"]