{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXL-K"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXL35K2V1B","FCQG50FVEB / RXL50K2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.3","1.6"]
["","Μέγ.","","kW","4.0","5.7"]
["","Ονομ.","","kW","3.40","5.00"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","460","700"]
["","EER","","","3.70","3.57"]
["","COP","","","3.56","3.87"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","B","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","4.20","6.00"]
["","Ελάχ.","","kW","1.3","1.6"]
["","Μέγ.","","kW","5.2","6.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]