{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":8,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","12.10","19.00","22.00"]
["Απόδοση θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","13.50","22.4","24.0"]
["Περίβλημα","Χρώμα","","","","Άβαφο","Άβαφο","Άβαφο"]
["","Υλικό","","","","Γαλβανισμένος χάλυβας","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","300","470","470"]
["","","","Πλάτος","mm","1,400","1,490","1,490"]
["","","","Βάθος","mm","700","1,100","1,100"]
["Βάρος","Μονάδα","","","kg","45","104","115"]
["Απαιτούμενο διάκενο ψευδοροφής >","mm","","","","350"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","Χαμηλή","m³/min","28.0","36.0","43.0"]
["","","Θέρμανση","Υψ.","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","Χαμηλή","m³/min","28.0","36.0","43.0"]
["","Εξωτερική στατική πίεση","","Υψ.","Pa","200","250","250"]
["","","","Ονομ.","Pa","50","62","62"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","66","69.0","71.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Χαμηλή","dBA","33","36.0","37.0"]
["","Θέρμανση","","Υψ.","dBA","40","43.0","44.0"]
["","","","Μέτρια","dBA","","39.0","40.0"]
["","","","Χαμηλή","dBA","33","36.0","37.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","15.90","19.1","22.2"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Ύψος αντλίας συμπυκνωμάτων","mm","","","","625"]
["Διακοσμητική μάσκα","Model","","","","BYBS125DJW1"]
["","Χρώμα","","","","Λευκό (10Y9/0.5)"]
["","Διαστάσεις","","Ύψος","mm","55"]
["","","","Πλάτος","mm","1,500"]
["","","","Βάθος","mm","500"]
["","Βάρος","","","kg","6.5"]
["Συστήματα ελέγχου","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","","1","1"]
["","Εγχειρίδιο εγκατάστασης και χειρισμού","","","","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","","1","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","1","1","1"]
["","Σωλήνα σύνδεσης αερίου","","","","","1","1"]
["","Υλικό σφικτήρα καλωδίου","","","","","1","1"]
["","Ροδέλα","","","","8","12","12"]
["","Ροδέλα γκρόβερ","","","","","2","2"]
["","Βίδα+Ροδέλα","","","","","45","45"]
["","Βίδα εξάγωνης κεφαλής με ροδέλα","","","","","49","49"]
["","Κοχλίες","","","","16","2","2"]
["","Βίδα εξάγωνης κεφαλής","","","","","2","2"]
["","Απλή ροδέλα","","","","","8","8"]
["Power supply","Όνομα","","","","","VE","VE"]
["","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60"]
["","Τάση","","","V","220-240/220","220-240/220","220-240/220"]
["Στάνταρτ εξαρτήματα","Ταινία εύκαμπτου σωλήνα","","","","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","1"]
["","Καλώδιο για συνήθη τροφοδοσία ισχύος","","","","2"]
["","Στεγανοποιητικό υλικό","","","","2"]
["","Θερμομονωτικός σωλήνας (υγρών)","","","","1"]
["","Θερμομονωτικός σωλήνας (αερίων)","","","","1"]
["Σημειώσεις","","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]