{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125B8W1B"]
["Απόδοση ψύξης","Ονομ.","","kW","12.50 (1)"]
["Συνδέσεις σωληνώσεων","Υγρού","OD","mm","9.52"]
["","Αερίου","Εξ.Διάμ.","mm","15.9"]
["","Συμπυκνωμάτων","OD","mm","26"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","2,075"]
["","EER","","","3.01"]
["","COP","","","3.79"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","B"]
["","","Θέρμανση","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","14.00 (2)"]
["Σημειώσεις","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 7,5m / υψομετρική διαφορά: 0m"]
["","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m / υψομετρική διαφορά: 0m"]
["","","","","(3) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]