{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQG125L7V1B","FDQ125C7VEB / RZQG125L7Y1B"]
["Απόδοση ψύξης","Ονομ.","","kW","12.0","12.0"]
["Ψύξη χώρου","SEER","","","5.61","5.61"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","748.663","748.663"]
["","Απόδοση","Pdesign","kW","12.00","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A+"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","12.71","12.71"]
["","SCOP/A","","","4.05","4.05"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","4,392","4,392"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","1,600","1,600"]
["","EER","","","3.75","3.75"]
["","COP","","","3.83","3.83"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","13.5","13.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]