{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQG125L8V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","12.0"]
["Ψύξη χώρου","SEER","","","5.81"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","722.892"]
["","Απόδοση","Pdesign","kW","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","12.71"]
["","SCOP/A","","","4.21"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","4,226.603"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","1,600"]
["","EER","","","3.75"]
["","COP","","","3.83"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","13.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]