{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L9V1B (Archived)","FDQ125C7VEB / RZQSG125L9V1B (Archived)"]
["Απόδοση ψύξης","Ονομ.","","kW","12.0","12.0"]
["Απόδοση θέρμανσης","Ονομ.","","kW","13.5","13.5"]
["Ονομαστική απόδοση","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Annual energy consumption","","kWh","1,870","1,870"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","B","B"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A"]
["","Απόδοση","Pdesign","kW","12.00","12.00"]
["","SEER","","","5.20","5.20"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","808","808"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A"]
["","Απόδοση","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.90","3.90"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,729","2,729"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]