{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / RXS25L3V1B","FDXM35F3V1B / RXS35L3V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","2.40","3.40"]
["Ψύξη χώρου","SEER","","","5.63","5.21"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","149","228"]
["","Απόδοση","Pdesign","kW","2.40","3.40"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","2.60","2.90"]
["","SCOP/A","","","4.24","3.88"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","858","1,047"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.50","9.50"]
["","Αποχέτευση","OD","mm","VP20 (Εξωτερική διάμ. 26, Εσωτερική διάμ. 20)","VP20 (Εξωτερική διάμ. 26, Εσωτερική διάμ. 20)"]
["Ονομαστική απόδοση","EER","","","3.74","2.96"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","321","574"]
["","COP","","","4.00","3.48"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","B"]
["","","Θέρμανση","","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","3.20","4.00"]
["Σημειώσεις","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]