{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","35.0","35.0","","38.0"]
["","","","Μέτρια","dBA","33.0","33.0","","35.0"]
["","","","Χαμηλή","dBA","27.0","27.0","","30.0"]
["","Ψύξη","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Χαμηλή","dBA","27.0","27.0","","30.0"]
["","","","Υψ.","dBA","35.0","35.0","","38.0"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","","1"]
["","Μόνωση συνδέσμου","","","","1","1","","1"]
["","Στεγανοποιητικό παρέμβυσμα","","","","1","1","","1"]
["","Μεταλλικός σφιγκτήρας","","","","1","1","","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","1","1","","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","","8","8","","8"]
["","Στεγανοποιητικό υλικό","","","","2","2","","2"]
["","Σφιγκτήρες","","","","6","6","","6"]
["","Έλασμα στερέωσης ροδέλας","","","","4","4","","4"]
["","Βίδες για φλάντζες αγωγών","","","","1","1","","1"]
["","Φίλτρο αέρα","","","","1","1","","1"]
["Συνδέσεις σωληνώσεων","Υγρού","","OD","mm","6.35","6.35","","6.35"]
["","Αερίου","","Εξ.Διάμ.","mm","9.50","9.50","","12.70"]
["","Συμπυκνωμάτων","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.036","0.036","","0.060"]
["","Θέρμανση","","Ονομ.","kW","0.036","0.036","","0.060"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53.0","53.0","","56.0"]
["","Θέρμανση","","","dBA","53.0","53.0","","56.0"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","750","750","","1,150"]
["","","","Βάθος","mm","620","620","","620"]
["","","","Ύψος","mm","200","200","","200"]
["Βάρος","Μονάδα","","","kg","21","21","","28"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Ονομ.","Pa","30","30","","40"]
["","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Χαμηλή","m³/min","7.3","7.3","","13.5"]
["","","Ψύξη","Χαμηλή","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Υψ.","m³/min","8.7","8.7","","16.0"]
["Power supply","Φάση","","","","1~","1~","","1~"]
["","Συχνότητα","","","Hz","50","50","","50"]
["","Τάση","","","V","220-240","220-240","","220-240"]
["Σημειώσεις","","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","0.060"]
["","Θέρμανση","","Ονομ.","kW","","","0.060"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","","200"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","","1150"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","","620"]
["Βάρος","Μονάδα","","","kg","","","28"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","15.8"]
["","","","Μέτρια","m³/min","","","14.6"]
["","","","Χαμηλή","m³/min","","","13.3"]
["","","Θέρμανση","Υψ.","m³/min","","","15.8"]
["","","","Μέτρια","m³/min","","","14.6"]
["","","","Χαμηλή","m³/min","","","13.3"]
["","Εξωτερική στατική πίεση","","Ονομ.","Pa","","","40"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","55.0"]
["","Θέρμανση","","","dBA","","","55.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","38.0"]
["","","","Μέτρια","dBA","","","35.0"]
["","","","Χαμηλή","dBA","","","30.0"]
["","Θέρμανση","","Υψ.","dBA","","","38.0"]
["","","","Μέτρια","dBA","","","35.0"]
["","","","Χαμηλή","dBA","","","30.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","12.70"]
["","Αποχέτευση","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Φίλτρο αέρα","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Τροφοδοσία ισχύος","Φάση","","","","","","1~"]
["","Συχνότητα","","","Hz","","","50"]
["","Τάση","","","V","","","220-240"]