{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG125L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L8Y1B"]
["Ψύξη χώρου","SEER","","","4.80","4.8","5.10","5.1","5.10","5.1"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","496","496","652","652","824","824"]
["","Απόδοση","Pdesign","kW","6.80","6.8","9.50","9.5","12.00","12"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","B","B","B","B","B","B"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","6.00","6","10.74","10.74","11.30","12.71"]
["","SCOP/A","","","3.80","3.8","3.80","3.8","3.80","3.8"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A","A","A","A","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,211","2,211","3,957","3,957","4,164","4,683"]
["Σημειώσεις","","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]