{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Στάθμη ηχ. πίεσης","Θέρμανση","","Υψ.","dBA","33.0","33.0","36.0","36.0"]
["","","","Ονομ.","dBA","31.0","31.0","33.0","33.0"]
["","","","Χαμηλή","dBA","28.0","28.0","30.0","30.0"]
["","Ψύξη","","Μέτρια","dBA","31.0","31.0","33.0","33.0"]
["","","","Χαμηλή","dBA","28.0","28.0","30.0","30.0"]
["","","","Υψ.","dBA","33.0","33.0","36.0","36.0"]
["Συστήματα ελέγχου","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Συνδέσεις σωληνώσεων","Υγρού","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35"]
["","Αερίου","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","12.7","12.7"]
["","Συμπυκνωμάτων","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53.0","53.0","56.0","56.0"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","790","790","1,190","1,190"]
["","","","Βάθος","mm","200","200","200","200"]
["","","","Ύψος","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Casing","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Colour","","","","Άβαφο","Άβαφο","Άβαφο","Άβαφο"]
["Βάρος","Μονάδα","","","kg","23.0","23.0","30.0","30.0"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Υψηλή","Pa","48","48","49","49"]
["","","","Ονομ.","Pa","30","30","40","40"]
["","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","8.7","8.7","16.0","16.0"]
["","","","Χαμηλή","m³/min","7.3","7.3","13.5","13.5"]
["","","","Ονομ.","m³/min","8.0","8.0","14.8","14.8"]
["","","Ψύξη","Χαμηλή","m³/min","7.3","7.3","13.5","13.5"]
["","","","Ονομ.","m³/min","8.0","8.0","14.8","14.8"]
["","","","Υψ.","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Φάση","","","","1~","1~","1~","1~"]
["","Όνομα","","","","VE","VE","VE","VE"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","","(1) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(1) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(1) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(1) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης"]
["","","","","","(2) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(2) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(2) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(2) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]