{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":11,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)","FTX50GV1B (Archived)","FTX60GV1B (Archived)","FTX71GV1B (Archived)"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","7.4","7.6","7.7","14.7","16.2","14.6"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","33","33","34","39","41","42"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Ονομ.","m³/min","7.8","8.0","8.4","13.9","15.1","16.9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","34","34","35","38","40","42"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","0.034","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["","Θέρμανση","","Ονομ.","kW","","","","0.036","0.045 (3) (4) (2), 0.045 (3) (4) (2), 0.045 (3) (4) (2)","0.060 (3) (2), 0.060 (3) (2), 0.06 (4)"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","283","283","283","290","290","290"]
["","","","Πλάτος","mm","770","770","770","1050","1050","1050"]
["","","","Βάθος","mm","198","198","198","238","238","238"]
["Βάρος","Μονάδα","","","kg","7","7","7","12","12","12"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.1","9.2","9.3","14.7","16.2","17.4"]
["","","","Χαμηλή","m³/min","5.9","6.0","6.1","10.3","11.4","11.6"]
["","","","Αθόρυβη λειτουργία","m³/min","4.7","4.8","4.9","9.5","10.2","10.6"]
["","","Θέρμανση","Υψ.","m³/min","9.4","9.7","10.1","16.1","17.4","19.7"]
["","","","Χαμηλή","m³/min","6.3","6.3","6.7","11.5","12.7","14.3"]
["","","","Αθόρυβη λειτουργία","m³/min","5.5","5.5","5.7","10.2","11.4","12.7"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","56","57","59","60","63"]
["","Θέρμανση","","","dBA","55","56","57","58","59","62"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","40","41","43","45","46"]
["","","","Χαμηλή","dBA","25","26","27","34","36","37"]
["","","","Αθόρυβη λειτουργία","dBA","22","22","23","31","33","34"]
["","Θέρμανση","","Υψ.","dBA","39","40","41","42","44","46"]
["","","","Χαμηλή","dBA","28","28","29","33","35","37"]
["","","","Αθόρυβη λειτουργία","dBA","25","25","26","30","32","34"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52","12.7","12.7","15.9"]
["","Αποχέτευση","","","","18","18","18","18","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","ARC433B70","ARC433B70","ARC433B70"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1","1","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","1","1","1","1","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","1","1","1","1"]
["","Μπαταρίες","","","","2","2","2","2","2","2"]
["","Βίδα συναρμογής της εσωτερικής μονάδας","","","","2","2","2"]
["","Πλάκα στήριξης","","","","1","1","1","1","1","1"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","1","1","1","1"]
["","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","","2","2","2","2","2","2"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1","V1","V1","V1","V1"]
["","Φάση","","","","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Στάνταρτ εξαρτήματα","Βίδες στερέωσης εσωτερικής μονάδας","","","","","","","2","2"]
["Σημειώσεις","","","","","","","","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα"]
["","","","","","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Στάνταρτ εξαρτήματα","Βίδες στερέωσης εσωτερικής μονάδας (M4x12L)","","","","","","","","","2"]