{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","39","40","41","","46"]
["","","","Μέτρια","dBA","32","33","33","","42"]
["","","","Αθόρυβη λειτουργία","dBA","19","19","19","","24"]
["","","","Χαμηλή","dBA","25","25","25","","33"]
["","Ψύξη","","Μέτρια","dBA","32","33","33","","39"]
["","","","Αθόρυβη λειτουργία","dBA","19","19","19","","24"]
["","","","Χαμηλή","dBA","25","25","25","","31"]
["","","","Υψ.","dBA","39","40","41","","46"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","1","","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","1","","1"]
["","Φίλτρο αέρα","","","","2","2","2","","2"]
["","Τηλεχειριστήριο υπερύθρων","","","","1","1","1","","1"]
["","Πλάκα στήριξης τηλεχειριστηρίου","","","","1","1","1","","1"]
["","Βιδωτή σακούλα","","","","1","1","1","","1"]
["","Βιδωτό κάλυμμα","","","","1","1","1","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2","2","2","","2"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","1","1","1","","1"]
["Ψυκτικό μέσο","GWP","","","","675.0","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50","9.50","9.50","","12.70"]
["","Drain","","","","18","18","18","","18"]
["Power input","Ψύξη","","Ονομ.","kW","0.020","0.022","0.023","","0.030"]
["","Θέρμανση","","Ονομ.","kW","0.020","0.020","0.022","","0.039"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","57","57","60","","60"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","798","798","798","","798"]
["","","","Βάθος","mm","189","189","189","","189"]
["","","","Ύψος","mm","295","295","295","","295"]
["Περίβλημα","Colour","","","","Λευκό","Λευκό","Λευκό","","Λευκό"]
["Βάρος","Μονάδα","","","kg","11.50","11.50","11.50","","11.50"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Μέτρια","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Χαμηλή","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Αθόρυβη λειτουργία","m³/min","4.5","4.5","4.5","","5.7"]
["","","Ψύξη","Χαμηλή","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Μέτρια","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Υψ.","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Αθόρυβη λειτουργία","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Όνομα","","","","V1","V1","V1","","V1"]
["","Συχνότητα","","","Hz","50","50","50","","50"]
["","Τάση","","","V","220-240","220-240","220-240","","220-240"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","0.028"]
["","Θέρμανση","","Ονομ.","kW","","","","0.036"]
["Περίβλημα","Χρώμα","","","","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","","","295"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","","","798"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","","","189"]
["Βάρος","Μονάδα","","","kg","","","","11.50"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","","13.1"]
["","","","Μέτρια","m³/min","","","","9.8"]
["","","","Χαμηλή","m³/min","","","","7.2"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","4.6"]
["","","Θέρμανση","Υψ.","m³/min","","","","14.6"]
["","","","Μέτρια","m³/min","","","","10.5"]
["","","","Χαμηλή","m³/min","","","","7.7"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","5.2"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","60"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","45"]
["","","","Μέτρια","dBA","","","","37"]
["","","","Χαμηλή","dBA","","","","29"]
["","","","Αθόρυβη λειτουργία","dBA","","","","21"]
["","Θέρμανση","","Υψ.","dBA","","","","45"]
["","","","Μέτρια","dBA","","","","37"]
["","","","Χαμηλή","dBA","","","","29"]
["","","","Αθόρυβη λειτουργία","dBA","","","","21"]
["Ψυκτικό μέσο","GWP","","","","","","","675.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","","12.70"]
["","Αποχέτευση","","","","","","","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","ARC466A58"]
["","Τηλεχειριστήριο με καλώδιο","","","","","","","BRC073"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Φίλτρο αέρα","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","","","V1"]
["","Φάση","","","","","","","1~"]
["","Συχνότητα","","","Hz","","","","50"]
["","Τάση","","","V","","","","220-240"]