{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","39","40"]
["","","Μέτρια","dBA","34","34"]
["","","Αθόρυβη λειτουργία","dBA","21","21"]
["","","Χαμηλή","dBA","28","28"]
["","Ψύξη","Μέτρια","dBA","33","33"]
["","","Αθόρυβη λειτουργία","dBA","20","20"]
["","","Χαμηλή","dBA","25","26"]
["","","Υψ.","dBA","39","40"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","1","1"]
["","Εγχειρίδιο χειρισμού","","","1","1"]
["","Τηλεχειριστήριο υπερύθρων","","","1","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","1","1"]
["","Πλάκα στήριξης","","","1","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","2","2"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35"]
["","Αερίου","Εξ.Διάμ.","mm","9.50","9.50"]
["","Drain","","","18","18"]
["Ισχύς εισόδου","Ψύξη","Ονομ.","kW","0.017","0.019"]
["","Θέρμανση","Ονομ.","kW","0.020","0.020"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","55","55"]
["","Θέρμανση","","dBA","55","55"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","770","770"]
["","","Βάθος","mm","225","225"]
["","","Ύψος","mm","286","286"]
["Περίβλημα","Χρώμα","","","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","kg","8.50","8.50"]
["Power supply","Φάση","","","1~","1~"]
["","Συχνότητα","","Hz","50","50"]
["","Τάση","","V","220-240","220-240"]