{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Power input","Ψύξη","","Ονομ.","kW","","","","","0.029","","0.032"]
["","Θέρμανση","","Ονομ.","kW","","","","","0.032","","0.035"]
["Περίβλημα","Χρώμα","","","","","","","","Λευκό","","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","","","","295","","295"]
["","","","Πλάτος","mm","","","","","990","","990"]
["","","","Βάθος","mm","","","","","263","","263"]
["Βάρος","Μονάδα","","","kg","","","","","13.5","","13.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","","","16.8","","17.3"]
["","","","Μέτρια","m³/min","","","","","14.4","","14.8"]
["","","","Χαμηλή","m³/min","","","","","11.9","","12.2"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","10.5","","10.7"]
["","","Θέρμανση","Υψ.","m³/min","","","","","17.3","","17.9"]
["","","","Μέτρια","m³/min","","","","","14.8","","15.8"]
["","","","Χαμηλή","m³/min","","","","","12.2","","12.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","10.7","","11.3"]
["Sound power level","Ψύξη","","","dBA","","","","","59","","62"]
["","Θέρμανση","","","dBA","","","","","61","","62"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","","43","","46"]
["","","","Μέτρια","dBA","","","","","39","","42"]
["","","","Χαμηλή","dBA","","","","","34","","37"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","31","","34"]
["","Θέρμανση","","Υψ.","dBA","","","","","42","","45"]
["","","","Μέτρια","dBA","","","","","38","","41"]
["","","","Χαμηλή","dBA","","","","","33","","36"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","30","","33"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","","6.35","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","","12.7","","12.7"]
["","Συμπυκνωμάτων","","","","","","","","18","","18"]
["Χειριστήρια","Infrared remote control","","","","","","","","ARC470A1","","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","","","","","BRC073A1","","BRC073A1"]
["Στάνταρτ εξαρτήματα","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","","","","","2","","2"]
["","Εγχειρίδιο εγκατάστασης","","","","","","","","1","","1"]
["","Εγχειρίδιο χειρισμού","","","","","","","","1","","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","","","","","1","","1"]
["","Υποδοχή τηλεχειριστηρίου","","","","","","","","1","","1"]
["","Πλάκα στήριξης","","","","","","","","1","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","","","","","2","","2"]
["Power supply","Όνομα","","","","","","","","V1","","V1"]
["","Φάση","","","","","","","","1~","","1~"]
["","Συχνότητα","","","Hz","","","","","50","","50"]
["","Τάση","","","V","","","","","220-240","","220-240"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.023","0.023","0.029","0.040","","0.032"]
["","Θέρμανση","","Ονομ.","kW","0.023","0.023","0.029","0.040","","0.035"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","286","286","286","286","","295"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","770","770","770","","990"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225","225","225","225","","263"]
["Βάρος","Μονάδα","","","kg","8","8","8.5","9.00","","13.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.8","10","11.5","12.6","","17.3"]
["","","","Μέτρια","m³/min","8","8","8","9","","14.8"]
["","","","Χαμηλή","m³/min","6","6.2","6.4","6.9","","12.2"]
["","","","Αθόρυβη λειτουργία","m³/min","4.3","4.3","4.4","4.9","","10.7"]
["","","Θέρμανση","Υψ.","m³/min","10.4","10.4","11.9","12.8","","17.9"]
["","","","Μέτρια","m³/min","8.3","8.4","8.6","8.8","","15.8"]
["","","","Χαμηλή","m³/min","6.2","6.4","6.5","6.7","","12.8"]
["","","","Αθόρυβη λειτουργία","m³/min","5.3","5.3","5.3","5.2","","11.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53","54","54","59.0","","60"]
["","Θέρμανση","","","dBA","55","55","56","59.0","","62"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","40","43","45.0","","45"]
["","","","Μέτρια","dBA","33","33","34","36.0","","41"]
["","","","Χαμηλή","dBA","25","26","27","30.0","","36"]
["","","","Αθόρυβη λειτουργία","dBA","20","20","20","22.0","","33"]
["","Θέρμανση","","Υψ.","dBA","39","40","40","44.0","","44"]
["","","","Μέτρια","dBA","34","34","35","34.0","","40"]
["","","","Χαμηλή","dBA","28","28","29","28.0","","35"]
["","","","Αθόρυβη λειτουργία","dBA","21","21","21","22.0","","32"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6","6","6","6","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5","9.5","9.50","","12.7"]
["","Αποχέτευση","","","","18","18","18","18","","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","","50"]
["","Τάση","","","V","220-440","220-440","220-440","220-440","","220-240"]
["","Όνομα","","","","","","","","","V1"]