{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","47","47"]
["","","Αθόρυβη λειτουργία","dBA","19","19"]
["","","Χαμηλή","dBA","23","23"]
["","Ψύξη","Αθόρυβη λειτουργία","dBA","21","21"]
["","","Χαμηλή","dBA","33","33"]
["","","Υψ.","dBA","45","45"]
["","","Ονομ.","dBA","37","36"]
["","Ψύξη","Ονομ.","dBA","39","39"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","1","1"]
["","Εγχειρίδιο χειρισμού","","","1","1"]
["","Τηλεχειριστήριο υπερύθρων","","","1","1"]
["","Μπαταρίες","","","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","1","1"]
["","Πλάκα στήριξης","","","1","1"]
["","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","2","2"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","2","2"]
["Χειριστήρια","Infrared remote control","","","ARC466A9","ARC466A9"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","9.5","9.5"]
["","Συμπυκνωμάτων","","","18","18"]
["Ισχύς εισόδου","Ψύξη","Ονομ.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Θέρμανση","Ονομ.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Ψύξη","","dBA","59","59"]
["","Θέρμανση","","dBA","62","62"]
["Διαστάσεις","Μονάδα","Πλάτος","χιλ.","900","900"]
["","","Βάθος","χιλ.","215","215"]
["","","Ύψος","χιλ.","298","298"]
["Casing","Colour","","","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","kg","12","12"]
["Power supply","Φάση","","","1~","1~"]
["","Συχνότητα","","Hz","50","50"]
["","Όνομα","","","V1","V1"]
["","Τάση","","V","220-240","220-240"]
["Σημειώσεις","","","","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί.","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]