{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RKS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RKS60F3V1B","FTXS71GV1B / RKS71FAV1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.7","2.3"]
["","Μέγ.","","kW","6.7","8.5"]
["","Ονομ.","","kW","6.0 (1)","7.1 (1)"]
["Συνδέσεις σωληνώσεων","Υγρού","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35"]
["","Αερίου","ΕΞ.ΔΙΑΜ.","mm","12.7","15.9"]
["","Συμπυκνωμάτων","OD","mm","18.0","18.0"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","995","1,175"]
["","EER","","","3.02","3.02"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","B","D"]
["Σημειώσεις","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m"]
["","","","","(2) - Οι τιμές απόδοσης αντιστοιχούν στις καθαρές τιμές και περιλαμβάνουν μικρή απόκλιση προς τα κάτω για τη λειτουργία ψύξης, που αντιστοιχεί στη θέρμανση του κινητήρα ανεμιστήρα της εσωτερικής μονάδας.","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","(3) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]