{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F8"]
[]
[]
[]
[]
["","","","","FTXS71GV1B / RXS71FAV1B8"]
["Απόδοση ψύξης","Ελάχ.","","kW","2.3"]
["","Μέγ.","","kW","8.5"]
["","Ονομ.","","kW","7.10"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","15.9"]
["","Συμπυκνωμάτων","OD","mm","18"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","1,175"]
["","EER","","","3.02"]
["","COP","","","3.22"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","B"]
["","","Θέρμανση","","C"]
["Απόδοση θέρμανσης","Ονομ.","","kW","8.20"]
["","Ελάχ.","","kW","2.3"]
["","Μέγ.","","kW","10.2"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - 220V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]