{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","40","","","","","","45"]
["","","","Αθόρυβη λειτουργία","dBA","19","","","","","","22"]
["","","","Χαμηλή","dBA","27","","","","","","33"]
["","Ψύξη","","Αθόρυβη λειτουργία","dBA","19","","","","","","21"]
["","","","Χαμηλή","dBA","24","","","","","","33"]
["","","","Υψ.","dBA","40","","","","","","45"]
["","","","Ονομ.","dBA","34","","","","","","39"]
["","Ψύξη","","Ονομ.","dBA","32","","","","","","39"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","","","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1","","","","","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","","","","","","1"]
["","Μπαταρίες","","","","2","","","","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","","","","","","1"]
["","Πλάκα στήριξης","","","","1","","","","","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","","","","","","2"]
["","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","","2","","","","","","2"]
["Χειριστήρια","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","","","","","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","9.5","","","","","","9.5"]
["","Συμπυκνωμάτων","","","","18","","","","","","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Θέρμανση","","Ονομ.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","58","","","","","","59"]
["","Θέρμανση","","","dBA","58","","","","","","59"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","780","","","","","","900"]
["","","","Βάθος","χιλ.","215","","","","","","215"]
["","","","Ύψος","χιλ.","289","","","","","","298"]
["Περίβλημα","Colour","","","","Λευκό","","","","","","Λευκό"]
["Βάρος","Μονάδα","","","kg","8","","","","","","11"]
["Power supply","Φάση","","","","1~","","","","","","1~"]
["","Συχνότητα","","","Hz","50","","","","","","50"]
["","Όνομα","","","","V1","","","","","","V1"]
["","Τάση","","","V","220-240","","","","","","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Θέρμανση","","Ονομ.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Περίβλημα","Χρώμα","","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","","215","289","215","298","215","","215","298","215"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","","780","780","780","900","900","","900","900","900"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","","289","215","289","215","298","","298","215","298"]
["Βάρος","Μονάδα","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Μέτρια","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Χαμηλή","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Αθόρυβη λειτουργία","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Θέρμανση","Υψ.","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Μέτρια","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Χαμηλή","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Αθόρυβη λειτουργία","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Θέρμανση","","","dBA","","58","58","58","59","59","","59","60","60"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Μέτρια","dBA","","32","33","33","","37","","39","","40"]
["","","","Χαμηλή","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Αθόρυβη λειτουργία","dBA","","19","19","19","19","19","","21","23","23"]
["","Θέρμανση","","Υψ.","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Μέτρια","dBA","","34","34","34","","39","","39","","40"]
["","","","Χαμηλή","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Αθόρυβη λειτουργία","dBA","","19","19","19","19","19","","22","24","24"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Αποχέτευση","","","","","18","18","18","18","18","","18","18","18"]
["Χειριστήρια","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Φάση","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Τάση","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","","","9.1","","11.2","","","","11.9"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","","","33","","37","","","","40"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Ονομ.","m³/min","","","8.0","","9.3","","","","10.8"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","","","34","","39","","","","40"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Στάνταρτ εξαρτήματα","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Σημειώσεις","","","","","","","","","","","(4) - 240V"]