{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","39","42","44"]
["","","","Αθόρυβη λειτουργία","dBA","19","19","24"]
["","","","Χαμηλή","dBA","28","29","31"]
["","Ψύξη","","Αθόρυβη λειτουργία","dBA","19","19","23"]
["","","","Χαμηλή","dBA","26","27","30"]
["","","","Υψ.","dBA","38","42","47"]
["","","","Ονομ.","dBA","35","36","38"]
["","Ψύξη","","Ονομ.","dBA","33","35","38"]
["Στάνταρτ εξαρτήματα","Φωτοκαταλυτικό φίλτρο καθαρισμού και με αποσμητική δράση","","","","1","1","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","1","1"]
["","Μπαταρίες ξηρού τύπου","","","","2","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","3","3","3"]
["","Πλάκα στήριξης","","","","1","1","1"]
["Control systems","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","9.5","9.5","9.5"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.030","0.030","0.030"]
["","Θέρμανση","","Ονομ.","kW","0.030","0.030","0.030"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","54","57","60"]
["","Θέρμανση","","","dBA","56","57","59"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","798","798","798"]
["","","","Βάθος","χιλ.","372","372","372"]
["","","","Ύψος","χιλ.","295","295","295"]
["Περίβλημα","Colour","","","","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","","kg","15","15","15"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","11.7","13.3","14.4"]
["","","","Χαμηλή","m³/min","6.7","6.9","7.7"]
["","","","Αθόρυβη λειτουργία","m³/min","4.8","4.8","5.9"]
["","","Ψύξη","Χαμηλή","m³/min","5.3","5.6","6.6"]
["","","","Υψ.","m³/min","10.7","12.1","15.0"]
["","","","Αθόρυβη λειτουργία","m³/min","4.0","4.0","4.6"]
["","","","Ονομ.","m³/min","8.6","9.2","10.7"]
["","","Ψύξη","Ονομ.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Όνομα","","","","V1","V1","V1"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Μπροστινή πλευρά εναλλάκτη θερμότητας","(4) - Μπροστινή πλευρά εναλλάκτη θερμότητας","(4) - Μπροστινή πλευρά εναλλάκτη θερμότητας"]
["","","","","","(5) - Όπισθεν πλευρά εναλλάκτη θερμότητας","(5) - Όπισθεν πλευρά εναλλάκτη θερμότητας","(5) - Όπισθεν πλευρά εναλλάκτη θερμότητας"]