{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","","","41","46","47"]
["","","","Μέτρια","dBA","","","","38","42","43"]
["","","","Χαμηλή","dBA","","","","35","39","40"]
["","Ψύξη","","Μέτρια","dBA","","","","38","42","43"]
["","","","Χαμηλή","dBA","","","","35","39","40"]
["","","","Υψ.","dBA","","","","41","46","47"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","","","","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","","","","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","","","","1","1","1"]
["","Θερμομονωτικός σωλήνας","","","","","","","3","3","3"]
["","Πλαστικός σφιγκτήρας","","","","","","","10","10","10"]
["","Ταινία εύκαμπτου σωλήνα","","","","","","","1","1","1"]
["","Στεγανοποιητικό υλικό","","","","","","","4","4","4"]
["","Έλασμα στερέωσης ροδέλας","","","","","","","1","1","1"]
["","Σύνδεσμος εξόδου συμπυκνωμάτων","","","","","","","1","1","1"]
["","Τύπου άνευ υφάνσεως","","","","","","","1","1","1"]
["","Ροδέλα","","","","","","","8","8","8"]
["","Βίδα συναρμογής του εύκαμπτου σωλήνα αποχέτευσης","","","","","","","5","5","5"]
["Χειριστήρια","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","","","","","","12.1"]
["Piping connections","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","15.9","15.9","15.9"]
["","Αποχέτευση","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","59","64","65"]
["","Θέρμανση","","","dBA","","","","59","64"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","","950","950","950"]
["","","","Βάθος","mm","","","","950","950","950"]
["","","","Ύψος","mm","","","","198","198","198"]
["Περίβλημα","Υλικό","","","","","","","Ρητίνη","Ρητίνη","Ρητίνη"]
["","Colour","","","","","","","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')"]
["Βάρος","Μονάδα","","","kg","","","","25.0","26.0","26"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","","","","23.0","31.0","32.5"]
["","","","Μέτρια","m³/min","","","","19.5","25.5","26.5"]
["","","","Χαμηλή","m³/min","","","","16.0","20.0","20.5"]
["","","Ψύξη","Χαμηλή","m³/min","","","","16.0","20.0","20.5"]
["","","","Μέτρια","m³/min","","","","19.5","25.5","26.5"]
["","","","Υψ.","m³/min","","","","23.0","31.0","32.5"]
["Ύψος αντλίας συμπυκνωμάτων","mm","","","","","","","600","600","600"]
["Απόδοση θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","","","","","","13.5"]
["Περίβλημα","Χρώμα","","","","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')"]
["","Υλικό","","","","Ρητίνη","Ρητίνη","Ρητίνη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","198","198","198"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","950","950","950"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","950","950","950"]
["Βάρος","Μονάδα","","","kg","25.0","26.0","26.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","23.0","31.0","32.5"]
["","","","Μέτρια","m³/min","19.5","25.5","26.5"]
["","","","Χαμηλή","m³/min","16.0","20.0","20.5"]
["","","Θέρμανση","Υψ.","m³/min","23.0","31.0","32.5"]
["","","","Μέτρια","m³/min","19.5","25.5","26.5"]
["","","","Χαμηλή","m³/min","16.0","20.0","20.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","59","64","65"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","41","46","47"]
["","","","Μέτρια","dBA","38","42","43"]
["","","","Χαμηλή","dBA","35","39","40"]
["","Θέρμανση","","Υψ.","dBA","41","46","47"]
["","","","Μέτρια","dBA","38","42","43"]
["","","","Χαμηλή","dBA","35","39","40"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.9","15.9","15.9"]
["","Αποχέτευση","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Ύψος αντλίας συμπυκνωμάτων-=-χιλ.","mm","","","","600","600","600"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","","","12.10"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","","","13.5"]