{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FUQ71CVEB / RZQG71L8V1B","FUQ100CVEB / RZQG100L8V1B","FUQ125CVEB / RZQG125L8V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","6.8","9.5","12.0"]
["Ψύξη χώρου","SEER","","","6.50","6.11","5.61"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","366.154","544.19","748.663"]
["","Απόδοση","Pdesign","kW","6.80","9.50","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++","A+"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","7.60","11.30","14.13"]
["","SCOP/A","","","4.20","4.50","4.44"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A+","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,533.333","3,515.556","4,456"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","840","1,230","1,770"]
["","EER","","","4.05","3.86","3.39"]
["","COP","","","4.08","3.95","3.42"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A"]
["","","Θέρμανση","","A","A","B"]
["Απόδοση σε λειτουργία θέρμανσης","Ονομ.","","kW","7.5","10.8","13.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]