{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","","","12.10","13.40"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","","","13.5","15.5"]
["Περίβλημα","Χρώμα","","","","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1850","","1850","1850"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","600","","600","600"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","270","","350","350"]
["Βάρος","Μονάδα","","","kg","42","50","50","50"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","18","28","28","30"]
["","","","Μέτρια","m³/min","16","25","26","28"]
["","","","Χαμηλή","m³/min","14","22","24","26"]
["","","Θέρμανση","Υψ.","m³/min","18","28","28","30"]
["","","","Μέτρια","m³/min","16","25","26","28"]
["","","","Χαμηλή","m³/min","14","22","24","26"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","62","63","65"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","43","50","51","53"]
["","","","Μέτρια","dBA","41","47","48","51"]
["","","","Χαμηλή","dBA","38","44","46","48"]
["","Θέρμανση","","Υψ.","dBA","43","50","51","53"]
["","","","Μέτρια","dBA","38","44","46","48"]
["","","","Ονομ.","dBA","41","47","48","51"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52","","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.9","","15.9","15.9"]
["","Αποχέτευση","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","1850"]
["","","","Πλάτος","mm","","600"]
["","","","Βάθος","mm","","350"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","15.9"]
["Σημειώσεις","","","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]