{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQSG71L3V1B","FVQ100CVEB / RZQSG100L9V1B","FVQ125CVEB / RZQSG125L9V1B","FVQ140CVEB / RZQSG140L9V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","6.8","9.5","12.0","13.4"]
["Ψύξη χώρου","SEER","","","5.50","5.50","5.50"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","433","605","764"]
["","Απόδοση","Pdesign","kW","6.80","9.50","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A","A"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","6.33","7.60","7.60"]
["","SCOP/A","","","3.86","4.01","3.85"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A+","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,296","2,654","2,764"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","1,060","1,480","2,135","2,225"]
["","EER","","","3.21","3.21","2.81","3.01"]
["","COP","","","3.61","3.61","3.41","3.41"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A"]
["","","Θέρμανση","","A","A","B"]
["Απόδοση θέρμανσης","Ονομ.","","kW","7.5","10.8","13.5","15.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]