{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.3","1.4","1.7"]
["","Ονομ.","","kW","2.5","3.5","5.0"]
["","Μέγ.","","kW","3.0","3.8","5.6"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.3","1.4","1.7"]
["","Ονομ.","","kW","3.4","4.5","5.8"]
["","Μέγ.","","kW","4.5","5.0","8.1"]
["Ονομαστική απόδοση","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","270","470","755"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A"]
["","","Θέρμανση","","A","A","A"]
["Συνδέσεις σωληνώσεων","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.5","9.5","12.7"]
["","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++","A"]
["","Απόδοση","Pdesign","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","134","189","324"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A+","A+"]
["","Απόδοση","Pdesign","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","842","1087","1543"]
["Σημειώσεις","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CWB; εξωτερική θερμοκρ. 35°CDB, 24°CWB","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CWB; εξωτερική θερμοκρ. 35°CDB, 24°CWB","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CWB; εξωτερική θερμοκρ. 35°CDB, 24°CWB"]
["","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB"]