{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.02","0.02","0.03"]
["","Θέρμανση","","Ονομ.","kW","0.02","0.03","0.03"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","600","600","600"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","750","750","750"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","238","238","238"]
["Βάρος","Μονάδα","","","kg","17","17","17"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","8.7","9.2","11.6"]
["","","","Μέτρια","m³/min","7","7","9"]
["","","","Χαμηλή","m³/min","4.9","4.9","6.6"]
["","","","Αθόρυβη λειτουργία","m³/min","4.1","4.1","5.4"]
["","","Θέρμανση","Υψ.","m³/min","9.2","9.8","12.8"]
["","","","Μέτρια","m³/min","7.2","7.2","10"]
["","","","Χαμηλή","m³/min","5.6","5.6","8.4"]
["","","","Αθόρυβη λειτουργία","m³/min","4.1","4.1","5.9"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","52","53","61"]
["","Θέρμανση","","","dBA","52","53","62"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","38","39","44"]
["","","","Μέτρια","dBA","32","32","38"]
["","","","Χαμηλή","dBA","25","25","31"]
["","","","Αθόρυβη λειτουργία","dBA","20","20","27"]
["","Θέρμανση","","Υψ.","dBA","38","39","46"]
["","","","Μέτρια","dBA","32","32","40"]
["","","","Χαμηλή","dBA","25","25","35"]
["","","","Αθόρυβη λειτουργία","dBA","19","19","29"]
["Ψυκτικό μέσο","GWP","","","","675","675","675"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.4","6.4","6.4"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5","12.7"]
["","Αποχέτευση","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1","V1"]
["","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m"]
["","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m"]
["Στάνταρτ εξαρτήματα","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]