{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDQ-M9"]
[]
[]
[]
[]
["","","","","FXDQ20M9V3B9","FXDQ25M9V3B9"]
["Ψυκτικό μέσο","Τύπος","","","R-410A","R-410A"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35"]
["","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","12.7","12.7"]
["","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση"]
["","Συμπυκνωμάτων","","","I.D. 21.6, O.D. 27.2","I.D. 21.6, O.D. 27.2"]
["Απαιτούμενο διάκενο ψευδοροφής >","mm","","","250","250"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","502","502"]
["","","Βάθος","mm","652","652"]
["","","Ύψος","mm","230","230"]
["Περίβλημα","Υλικό","","","Γαλβανισμένος χάλυβας","Γαλβανισμένος χάλυβας"]
["","Χρώμα","","","Άβαφο","Άβαφο"]
["Βάρος","Μονάδα","","kg","17","17"]
["Power supply","Φάση","","","1~","1~"]
["","Συχνότητα","","Hz","50","50"]
["","Όνομα","","","V1","V1"]
["","Τάση","","V","230","230"]
["Σημειώσεις","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 7,5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 7,5m / υψομετρική διαφορά: 0m"]
["","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m / υψομετρική διαφορά: 0m","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m / υψομετρική διαφορά: 0m"]