{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HXHD-A8"]
[]
[]
[]
[]
["","","","","","HXHD125A8V1B","HXHD200A8Y1B"]
["Περίβλημα","Χρώμα","","","","Γκρι μεταλλικό","Γκρι μεταλλικό"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","705","705"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","600","600"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","695","695"]
["Βάρος","Μονάδα","","","kg","92","147"]
["Ψυκτικό μέσο","Τύπος","","","","R-134a","R-134a"]
["","Φορτίο","","","kg","2","2.6"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","55","60"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","42, 43","46, 46"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","25","25"]
["","","","Μέγ.","°C","80.0","80.0"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","3~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","380-415"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","20","16"]
["Σημειώσεις","","","","","(1) - EW 40°C; LW 45°C; Dt 5°C; συνθήκες περιβάλλοντος: 7°CDB/6°CWB","(1) - EW 40°C; LW 45°C; Dt 5°C; συνθήκες περιβάλλοντος: 7°CDB/6°CWB"]
["","","","","","(2) - Για το νερό Dt 5°C","(2) - Για το νερό Dt 10°C"]
["","","","","","(3) - Τα επίπεδα θορύβου μετριώνται σε: EW 55°C; LW 65°C","(3) - Τα επίπεδα θορύβου μετριώνται σε: EW 55°C; LW 65°C"]
["","","","","","(4) - Τα επίπεδα θορύβου μετριώνται σε: EW 70°C; LW 80°C","(4) - Τα επίπεδα θορύβου μετριώνται σε: EW 70°C; LW 80°C"]
["","","","","","(5) - Ρύθμιση επί τόπου","(5) - Ρύθμιση επί τόπου"]
["","","","","","(6) - Σύμφωνα με το EN/IEC 61000-3-11, ενδέχεται να είναι απαραίτητο να συμβουλευθείτε το διαχειριστή δικτύου διανομής προκειμένου να διασφαλίσετε ότι ο εξοπλισμός είναι συνδεδεμένος μόνο σε δίκτυο τροφοδοσίας με Zsys (σύνθετη αντίσταση συστήματος) μικρότερο ή ίσο με Zmax","(6) - Σύμφωνα με το EN/IEC 61000-3-11, ενδέχεται να είναι απαραίτητο να συμβουλευθείτε το διαχειριστή δικτύου διανομής προκειμένου να διασφαλίσετε ότι ο εξοπλισμός είναι συνδεδεμένος μόνο σε δίκτυο τροφοδοσίας με Zsys (σύνθετη αντίσταση συστήματος) μικρότερο ή ίσο με Zmax"]
["","","","","","(7) - Ευρωπαϊκό/Διεθνές τεχνικό πρότυπο για τα όρια των μεταβολών τάσης,  διακυμάνσεων τάσεις και αναβόσβημα που παράγονται από δημόσιο σύστημα χαμηλής τάσης με ρεύμα εισόδου  ≤  75A.","(7) - Ευρωπαϊκό/Διεθνές τεχνικό πρότυπο για τα όρια των μεταβολών τάσης,  διακυμάνσεων τάσεις και αναβόσβημα που παράγονται από δημόσιο σύστημα χαμηλής τάσης με ρεύμα εισόδου  ≤  75A."]
["","","","","","(8) - Zsys: Αντίσταση συστήματος","(8) - Zsys: Αντίσταση συστήματος"]
["","","","","","(9) - Ισχύς βραχυκυκλώσεως","(9) - Ισχύς βραχυκυκλώσεως"]