{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1"]
["","Σωλήνες σύνδεσης","","","","1"]
["","Ετικέτα ψυκτικού μέσου για τη ρύθμιση του αερίου F","","","","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","1"]
["Βάρος","Μονάδα","","","kg","370"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Φορτίο","","","kg","11.5"]
["","Τύπος","","","","R-410A"]
["Κινητήρας ανεμιστήρα","Έξοδος","","","W","750"]
["","Μετάδοση κίνησης","","","","Άμεσης οδήγησης"]
["Εναλλάκτης θερμότητας","Τύπος","","","","Στοιχείο διασταυρούμενων πτερυγίων"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","1,240"]
["","","","Βάθος","mm","765"]
["","","","Ύψος","mm","1,680"]
["Περίβλημα","Colour","","","","Κρεμ_"]
["Ανεμιστήρας","Type","","","","Ανεμιστήρας έλικας"]
["","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","230"]
["","Ποσότητα","","","","2"]
["Power supply","Φάση","","","","3~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","380-415"]
["Σημειώσεις","","","","","(1) - λειτουργία προτεραιότητας ψύξης: εσωτερική θερμοκρ. 27°CDB, 19°CWB εξωτερική θερμοκρ. 32°CDB μήκος σωληνώσεων: 7,5m υψομετρική διαφορά: 0m"]
["","","","","","(2) - λειτουργία προτεραιότητας ψύξης: θερμοκρασία εξάτμισης -10°C εξωτερική θερμοκρ. 32°CDB Αναρρόφηση SH: 10°C"]
["","","","","","(3) - Λειτουργία ανάκτησης θερμότητας 100%: εσωτερική θερμοκρ. 20°CDB εξωτερική θερμοκρ. 7°CDB, 6°CWB φορτίο ψύξης 18kW μήκος σωληνώσεων: 7,5m υψομετρική διαφορά: 0m"]
["","","","","","(4) - Θερμοκρασία κορεσμού αντίστοιχη με την πίεση αναρρόφησης (πλευρά ψύξης): -10°C (σε συνθήκες ψύξης) απόδοση σύνδεσης για εσωτερικό κλιματιστικό: 10HP, όταν η ανάκτηση θερμότητας είναι 100%"]
["","","","","","(5) - Συμπιεστής 1"]
["","","","","","(6) - Συμπιεστής 2"]
["","","","","","(7) - Συμπιεστής 3"]
["","","","","","(8) - Πλήρωση της μονάδας από το εργοστάσιο"]
["","","","","","(9) - Εγκαταστήστε την παγίδα ελαίου στα 5m από την εξωτερική μονάδα"]
["","","","","","(10) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας"]
["","","","","","(11) - Για περισσότερες λεπτομέρειες σχετικά με τα στάνταρ αξεσουάρ, ανατρέξτε στο εγχειρίδιο εγκατάστασης/ λειτουργίας"]
["","","","","","(12) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]