{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Τύπος","","","","","Ιονιστής με λειτουργία ύγρανσης"]
["Εφαρμογή","","","","","Τύπου δαπέδου"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","700"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","270"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","270"]
["Βάρος","Μονάδα","","","kg","9.5"]
["Κατάλληλο εμβαδόν δωματίου","m²","","","","41 (1), 82 (2)"]
["CADR","m³/ώρα","","","","320"]
["Λειτουργία φιλτραρίσματος αέρα","Ισχύς εισόδου","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","ΧΑΜ.","kW","0.010"]
["","","","Αθόρυβο","kW","0.007"]
["Λειτουργία ύγρανσης","Ισχύς εισόδου","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","ΧΑΜ.","kW","0.014"]
["","","","Αθόρυβο","kW","0.011"]
["","Χωρητικότητα δεξαμενής νερού","","","l","2.7"]
["Στάθμη ηχητικής πίεσης","Λειτουργία φιλτραρίσματος αέρα","","Turbo","dBA","53.0"]
["","","","Μέτρια","dBA","39.0"]
["","","","Χαμηλή","dBA","29.0"]
["","","","Αθόρυβο","dBA","19.0"]
["","Λειτουργία ύγρανσης","","Turbo","dBA","53.0"]
["","","","Μέτρια","dBA","39.0"]
["","","","Χαμηλή","dBA","33.0"]
["","","","Αθόρυβο","dBA","25.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Λειτουργία φιλτραρίσματος αέρα","Turbo","m³/ώρα","330"]
["","","","Μέτρια","m³/ώρα","192"]
["","","","Χαμηλή","m³/ώρα","120"]
["","","","Αθόρυβο","m³/ώρα","54"]
["","","Λειτουργία ύγρανσης","Turbo","m³/ώρα","330"]
["","","","Μέτρια","m³/ώρα","192"]
["","","","Χαμηλή","m³/ώρα","144"]
["","","","Αθόρυβο","m³/ώρα","102"]
["Μέθοδος συλλογής σκόνης","","","","","Ηλεκτροστατικό φίλτρο HEPA"]
["Μέθοδος απόσμησης","","","","","Flash streamer + Καταλύτης με αποσμητική δράση"]
["Στάνταρτ εξαρτήματα","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Καλώδιο τροφοδοσίας","Καλώδιο τροφοδοσίας","","","","1.8"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Τροφοδοσία ισχύος-=-Συχνότητα","","Συχνότητα","","50/60"]
["","Τροφοδοσία ισχύος-=-Τάση","","Τάση","","220-240/220-230"]
["Ρεύμα λειτουργίας","Λειτουργία φιλτραρίσματος αέρα","Ρεύμα λειτουργίας-=-Λειτουργία φιλτραρίσματος αέρα-=-Turbo","Turbo","","0.50"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία φιλτραρίσματος αέρα-=-Μέτρια","Μέτρια","","0.19"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία φιλτραρίσματος αέρα-=-Χαμηλή","Χαμηλή","","0.12"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία φιλτραρίσματος αέρα-=-Αθόρυβο","Αθόρυβο","","0.09"]
["","Λειτουργία ύγρανσης","Ρεύμα λειτουργίας-=-Λειτουργία ύγρανσης-=-Turbo","Turbo","","0.50"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία ύγρανσης-=-Μέτρια","Μέτρια","","0.20"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία ύγρανσης-=-Χαμηλή","Χαμηλή","","0.15"]
["","","Ρεύμα λειτουργίας-=-Λειτουργία ύγρανσης-=-Αθόρυβο","Αθόρυβο","","0.13"]
["Σημειώσεις","","","","","(1) - Το κατάλληλο εμβαδόν δωματίου αρμόζει για τη λειτουργία μονάδας σε μέγιστη ταχύτητα ανεμιστήρα (HH). Ο χώρος δωματίου εφαρμογής υποδεικνύει το χώρο όπου συγκεκριμένη ποσότητα σωματιδίων σκόνης μπορεί να απομακρυνθεί μέσα σε 30 λεπτά. (JEM 1467)"]
["","","","","","(2) - Μετατροπή στα πρότυπα NRCC από τιμές δοκιμών σε συμφωνία με το JEM1467."]