{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","30.6","30.6"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","27.2","27.2"]
["","","","Εξαιρετικά χαμηλές","cfm","1080","1080"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","960","960"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","858","858"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","330","330"]
["Βάρος","Μονάδα","","","kg","40","40"]
["Συμπιεστής","Type","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10"]
["","","","Μέγ.","°CDB","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-25","-25"]
["","","","Μέγ.","°CWB","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","48","48"]
["","","","Χαμηλή","dBA","44","44"]
["","Θέρμανση","","Υψ.","dBA","49","49"]
["","","","Χαμηλή","dBA","45","45"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A"]
["","Φορτίο","","","kg","1","1"]
["","Φορτίο","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΣ.","Μέγ.","m","15","15"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]