{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A9"]
[]
[]
[]
[]
["","","","","","RXM25A5V1B9","RXM35A5V1B9","RXM50A5V1B9"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","610","","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","923","","954"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","367","","401"]
["Βάρος","Μονάδα","","","kg","36","36","49"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","600","","500"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10"]
["","","","Μέγ.","°CDB","50","50","46 (1)"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-21","-21","-15 (1)"]
["","","","Μέγ.","°CWB","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","47","48"]
["","Θέρμανση","","Ονομ.","dBA","47","49","49"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","Φορτίο","","","kg","0.95","0.95","1.10"]
["","Φορτίο","","","tCO2Eq","0.65","0.65","0.75"]
["","GWP","","","","675","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15","20"]
["Στάνταρτ εξαρτήματα","RXM25A5V1B9","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","610"]
["","","","Πλάτος","mm","","923"]
["","","","Βάθος","mm","","367"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","rpm","","600"]
["Στάνταρτ εξαρτήματα","RXM35A5V1B9","","","","","1"]