{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M"]
[]
[]
[]
[]
["","","","","","RXM20M2V1B","RXM25M2V1B","RXM35M2V1B","RXM42M2V1B","RXM50M2V1B","RXM50MV1B","RXM60M2V1B","RXM71M2V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550","550","735","735","735","735","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","765","765","765","825","825","825","825","870"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","285","285","285","300","300","300","300","320"]
["Βάρος","Μονάδα","","","kg","32","32","32","47","47","44","44","56"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10","-10 (1)","-10 (1)","-10","-10","-10"]
["","","","Μέγ.","°CDB","46","46","46","46 (1)","46 (1)","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18","18","18","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46","49","","","48","48"]
["","","","Ονομ.","dBA","","","","48","48","","","47"]
["","","","Χαμηλή","dBA","","","","","","44","44"]
["","Θέρμανση","","Υψ.","dBA","47","47","49","","","49","49"]
["","","","Ονομ.","dBA","","","","48","49","","","48"]
["","","","Χαμηλή","dBA","","","","","","45","45"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Φορτίο","","","kg","0.76","0.76","0.76","1.30","1.40","1.4","1.45","1.15"]
["","Φορτίο","","","tCO2Eq","0.5","0.5","0.5","0.88","0.95","0.9","1.0","0.78"]
["","GWP","","","","675","675","675","675","675","675","675","675.0"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","30","30","30","30","30","30","30","30.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","20","20","20","20","20","20","20","20.0"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Στάνταρτ εξαρτήματα","Drain plug","","","","","","","1","1","","","1"]
["Σημειώσεις","","","","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["Στάνταρτ εξαρτήματα","Drain cap","","","","","","","","","","","3"]