{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Στάθμη ηχ. πίεσης","Θέρμανση","","Υψ.","dBA","49","","","52"]
["","","","Χαμηλή","dBA","46","","","49"]
["","Ψύξη","","Χαμηλή","dBA","46","","","49"]
["","","","Υψ.","dBA","49","","","52"]
["Στάνταρτ εξαρτήματα","Υποδοχή εξόδου συμπυκνωμάτων","","","","1","","","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Φορτίο","","","kg","1.5","","","2.3"]
["","Τύπος","","","","R-410A","","","R-410A"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","20","","","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","825","","","900"]
["","","","Βάθος","mm","300","","","320"]
["","","","Ύψος","mm","735","","","770"]
["Βάρος","Μονάδα","","","kg","48","","","71"]
["Power supply","Φάση","","","","1~","","","1~"]
["","Συχνότητα","","","Hz","50","","","50"]
["","Τάση","","","V","220-240","","","220-240"]
["Σημειώσεις","","","","","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","(1) - 220V","","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","(1) - 220V"]
["","","","","","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - 230V","","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - 230V"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","735","735","","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","825","825","","900","900"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","300","300","","320","320"]
["Βάρος","Μονάδα","","","kg","","48","48","","71","71"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","-10","-10","","-10","-10"]
["","","","Μέγ.","°CDB","","46","46","","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15","-15","","-15","-15"]
["","","","Μέγ.","°CWB","","18","20","","18","20"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","49","49","","52","52"]
["","","","Χαμηλή","dBA","","46","46","","49","49"]
["","Θέρμανση","","Υψ.","dBA","","49","49","","52","52"]
["","","","Χαμηλή","dBA","","46","46","","49","49"]
["Ψυκτικό μέσο","Τύπος","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Φορτίο","","","kg","","1.5","1.5","","2.3","2.3"]
["","Φορτίο","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","30","30","","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","20","20","","20","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~","1~","","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","","50","50"]
["","Τάση","","","V","","220-240","220-240","","220-240","220-240"]
["Σημειώσεις","","","","","","(3) - 240V","","","(3) - 240V"]
["Στάνταρτ εξαρτήματα","Drain socket","","","","","","1","","","1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","65"]