{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","","48"]
["","Ψύξη","","Υψ.","dBA","","","48"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","","","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","","","1"]
["","Τάπα αποχέτευσης (μόνο μοντέλα αντλιών θερμότητας)","","","","","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Φορτίο","","","kg","","","1.2"]
["","Τύπος","","","","","","R-410A"]
["Fan motor","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","rpm","","","780"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","rpm","","","740"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","","","46"]
["","","","Ελάχ.","°CDB","","","-10"]
["","Θέρμανση","Περιβάλλοντος","Μέγ.","°CWB","","","18"]
["","","","Ελάχ.","°CWB","","","-15"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","765"]
["","","","Βάθος","mm","","","285"]
["","","","Ύψος","mm","","","550"]
["Συμπιεστής","Τύπος","","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Βάρος","Μονάδα","","","kg","","","34"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","","904"]
["","","","Εξαιρετικά χαμηλές","m³/min","","","25.6"]
["","","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","","30.1"]
["","","","Εξαιρετικά χαμηλές","cfm","","","1,063"]
["Power supply","Φάση","","","","","","1~"]
["","Συχνότητα","","","Hz","","","50"]
["","Τάση","","","V","","","220-240"]
["Σημειώσεις","","","","","","","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","30.1","30.1"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","25.6","25.6"]
["","","","Εξαιρετικά χαμηλές","cfm","1063","1063"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","904","904"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","765","765"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","285","285"]
["Βάρος","Μονάδα","","","kg","34","34"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","780","780"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","740","740"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10"]
["","","","Μέγ.","°CDB","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15"]
["","","","Μέγ.","°CWB","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46"]
["","Θέρμανση","","Υψ.","dBA","47","47"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A"]
["","Φορτίο","","","kg","1.0","1.0"]
["","Φορτίο","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Σημειώσεις","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Στάνταρτ εξαρτήματα","Drain plug (only heat pump models)","","","","","1"]