{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","","48","48","50","50"]
["","Ψύξη","","Υψ.","dBA","","","48","48","49","49"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","","","1","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","","","1","1","1","1"]
["Ψυκτικό μέσο","GWP","","","","","","675","675","675","675"]
["","Charge","","","kg","","","1.34","1.34","1.34","1.34"]
["","Τύπος","","","","","","R-32","R-32","R-32","R-32"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","","","43","43","43","43"]
["","","","Ελάχ.","°CDB","","","-10","-10","-10","-10"]
["","Θέρμανση","Περιβάλλον","Μέγ.","°CWB","","","18","18","18","18"]
["","","","Ελάχ.","°CWB","","","-20","-20","-20","-20"]
["Piping connections","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","8","8","8","8"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","795","795","795","795"]
["","","","Βάθος","mm","","","300","300","300","300"]
["","","","Ύψος","mm","","","693","693","693","693"]
["Συμπιεστής","Τύπος","","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Βάρος","Μονάδα","","","kg","","","50","50","50","50"]
["Power supply","Φάση","","","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","","","50","50","50","50"]
["","Τάση","","","V","","","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","693","693"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","795","795"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","300","300"]
["Βάρος","Μονάδα","","","kg","50","50"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10"]
["","","","Μέγ.","°CDB","43","43"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-20","-20"]
["","","","Μέγ.","°CWB","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46"]
["","Θέρμανση","","Υψ.","dBA","46","46"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32"]
["","Φορτίο","","","kg","1.34","1.34"]
["","Φορτίο","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","10","10"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","8","8"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]