{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","870","870"]
["","","","Πλάτος","mm","1,100","1,100"]
["","","","Βάθος","mm","460","460"]
["Βάρος","Μονάδα","","","kg","117","117"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός, σπειροειδής συμπιεστής","Ερμητικά κλειστός, σπειροειδής συμπιεστής"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-20","-20"]
["","","","Μέγ.","°CDB","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-20","-20"]
["","","","Μέγ.","°CWB","15","15"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","73","76"]
["","Θέρμανση","","","dBA","76 (1)","79 (1)"]
["Στάθμη ηχ. πίεσης","Ψύξη","","Ονομ.","dBA","53","57"]
["","Θέρμανση","","Ονομ.","dBA","60","63"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32"]
["","Φορτίο","","","kg","5","5"]
["","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Υγρού","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52"]
["","Αερίου","","ΕΞ.ΔΙΑΜ.","mm","22.2","22.2"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","100","100"]
["","","Σύστημα","Χωρίς φορτίο","m","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","1","1"]
["","Πλαστικός σφιγκτήρας","","","","2","2"]
["","Αφαιρούμενη ετικέτα αερίου F","","","","1","1"]
["","Σωλήνες σύνδεσης","","","","6","6"]
["Power supply","Φάση","","","","3~","3~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","380-415","380-415"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","20","20"]
["Σημειώσεις","","","","","(1) - Σύμφωνα με ENER Lot 21","(1) - Σύμφωνα με ENER Lot 21"]