{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","","","","52"]
["","Ψύξη","","Ονομ.","dBA","","","","51"]
["Στάνταρτ εξαρτήματα","Πλαστικός σφιγκτήρας","","","","","","","2"]
["","Εγχειρίδιο εγκατάστασης","","","","","","","1"]
["","Ετικέτα ψυκτικού μέσου για τη ρύθμιση του αερίου F","","","","","","","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","","","","1"]
["","Ενεργειακή σήμανση LOT10","","","","","","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Φορτίο","","","kg","","","","3.75"]
["","Τύπος","","","","","","","R-32"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","9.52"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","","","85"]
["","","Σύστημα","Χωρίς φορτίο","m","","","","40"]
["","","","Ισοδύναμο","m","","","","100"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","15.9"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΣ.","Μέγ.","m","","","","0.5"]
["","","ΕΣ.-ΕΞ.","Μέγ.","m","","","","30.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","","Βλ. εγχειρίδιο εγκατάστασης"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","70"]
["","Θέρμανση","","","dBA","","","","70 (1)"]
["Συμπιεστής","Type","","","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","","","","940"]
["","","","Βάθος","χιλ.","","","","320"]
["","","","Ύψος","χιλ.","","","","1,430"]
["Βάρος","Μονάδα","","","kg","","","","92"]
["Power supply","Φάση","","","","","","","1~"]
["","Συχνότητα","","","Hz","","","","50"]
["","Τάση","","","V","","","","220-240"]
["Σημειώσεις","","","","","","","","(1) - Σύμφωνα με ENER Lot 21"]
["","","","","","","","","(2) - Ευρωπαϊκό/ διεθνές τεχνικό πρότυπο για τον καθορισμό των ορίων αρμονικών ρευμάτων που παράγει εξοπλισμός συνδεδεμένος σε δημόσιο δίκτυο χαμηλής τάσης με ρεύμα εισόδου μεγαλύτερο από 16A και ≤  75A ανά φάση."]
["","","","","","","","","(3) - Ssc: Ισχύς βραχυκυκλώσεως"]
["","","","","","","","","(4) - Ευρωπαϊκό/ διεθνές τεχνικό πρότυπο για τον καθορισμό των ορίων αρμονικών ρευμάτων που παράγει εξοπλισμός συνδεδεμένος σε δημόσιο δίκτυο χαμηλής τάσης με ρεύμα εισόδου  ≤  16A ανά φάση."]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","990","1430","1430"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","940","940","940"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","320","320","320"]
["Βάρος","Μονάδα","","","kg","70","92","92"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-20","-20","-20"]
["","","","Μέγ.","°CDB","52","52","52"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-20","-20","-20"]
["","","","Μέγ.","°CWB","18.0","18.0","18.0"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","64","66","69"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","47","50"]
["","Θέρμανση","","Ονομ.","dBA","49","51","52"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","Φορτίο","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Φορτίο","","","tCO2Eq","1.99","2.53","2.53"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","15.9","15.9","15.9"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","55","85","85"]
["","","Σύστημα","Ισοδύναμο","m","75","100","100"]
["","","","Χωρίς φορτίο","m","40","40","40"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30.0","30.0","30.0"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","0.5","0.5","0.5"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","20","32","32"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","","dBA","","","69 (1)"]
["Σημειώσεις","","","","","","","(1) - Σύμφωνα με ENER Lot 21"]