{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","12.10"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","13.5"]
["Περίβλημα","Χρώμα","","","","Fresh white ('κατάλευκο')"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1850"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","600"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","350"]
["Βάρος","Μονάδα","","","kg","50"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","28"]
["","","","Μέτρια","m³/min","26"]
["","","","Χαμηλή","m³/min","24"]
["","","Θέρμανση","Υψ.","m³/min","28"]
["","","","Μέτρια","m³/min","26"]
["","","","Χαμηλή","m³/min","24"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","63"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","51"]
["","","","Μέτρια","dBA","48"]
["","","","Χαμηλή","dBA","46"]
["","Θέρμανση","","Υψ.","dBA","51"]
["","","","Μέτρια","dBA","46"]
["","","","Ονομ.","dBA","48"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.9"]
["","Αποχέτευση","","","","I.D. 20/O.D. 26"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50/60"]
["","Τάση","","","V","220-240/220"]