{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","38"]
["","","Μέτρια","dBA","36"]
["","","Χαμηλή","dBA","30"]
["","Ψύξη","Μέτρια","dBA","36"]
["","","Χαμηλή","dBA","30"]
["","","Υψ.","dBA","38"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","1"]
["","Εγχειρίδιο χειρισμού","","","1"]
["","Μόνωση συνδέσμου","","","1"]
["","Στεγανοποιητικό παρέμβυσμα","","","1"]
["","Μεταλλικός σφιγκτήρας","","","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","8"]
["","Στεγανοποιητικό υλικό","","","2"]
["","Σφιγκτήρες","","","6"]
["","Έλασμα στερέωσης ροδέλας","","","4"]
["","Βίδες για φλάντζες αγωγών","","","1"]
["","Φίλτρο αέρα","","","1"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","12.7"]
["","Συμπυκνωμάτων","","","VP20 (I.D. 20/O.D. 26)"]
["Ισχύς εισόδου","Ψύξη","Ονομ.","kW","0.060"]
["","Θέρμανση","Ονομ.","kW","0.060"]
["Sound power level","Ψύξη","","dBA","55"]
["","Θέρμανση","","dBA","55"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","1,150"]
["","","Βάθος","mm","620"]
["","","Ύψος","mm","200"]
["Βάρος","Μονάδα","","kg","30.0"]
["Fan","Εξωτερική στατική πίεση","Ονομ.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Συχνότητα","","Hz","50/60"]
["","Όνομα","","","VE"]
["","Τάση","","V","220-240"]
["Σημειώσεις","","","","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί."]